* Camera notes :

In “NXP\_Cup\_Car\_Implementation\_20180816.pdf” slide 27: It would be better if we store wether a left or right turn until we detect 2 borders.

In <https://community.nxp.com/docs/DOC-1058> : Exposure Time: 267µS to 68mS, other values are given in <https://community.nxp.com/docs/DOC-1030> (read the “Know your Settings” section, that marking tip seems to be useful ; read “Know your Zone” as well)

<https://community.nxp.com/docs/DOC-1030> : Read the Pro camera tips ... very useful